Device is Ready Port Read

|  |  |  |
| --- | --- | --- |
|  |  |  |

866

Data Port

|  |  |
| --- | --- |
| 0100 | 0001 |

866